SYSTEM DE2_Board
{
   System_Wizard_Version = "5.00";
   System_Wizard_Build = "168";
   WIZARD_SCRIPT_ARGUMENTS 
   {
      device_family = "CYCLONEII";
      clock_freq = "50000000";
      generate_hdl = "1";
      generate_sdk = "0";
      do_build_sim = "0";
      hdl_language = "verilog";
      view_master_columns = "1";
      view_master_priorities = "0";
      board_class = "";
      name_column_width = "75";
      desc_column_width = "75";
      bustype_column_width = "0";
      base_column_width = "75";
      end_column_width = "75";
      view_frame_window = "91:55:1157:939";
      do_log_history = "0";
      BOARD_INFO 
      {
         altera_avalon_cfi_flash 
         {
            reference_designators = "";
         }
         altera_avalon_epcs_flash_controller 
         {
            reference_designators = "U30";
         }
      }
      CLOCKS 
      {
         clk = "50000000";
      }
      device_family_id = "CYCLONEII";
      hardcopy_compatible = "0";
      clock_column_width = "74";
   }
   MODULE cpu_0
   {
      class = "altera_nios2";
      class_version = "5.0";
      iss_model_name = "altera_nios2";
      HDL_INFO 
      {
         PLI_Files = "";
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/cpu_0_test_bench.v, __PROJECT_DIRECTORY__/cpu_0.v";
         Synthesis_Only_Files = "";
      }
      MASTER instruction_master
      {
         PORT_WIRING 
         {
            PORT i_address
            {
               direction = "output";
               type = "address";
               width = "23";
               Is_Enabled = "1";
            }
            PORT i_read
            {
               direction = "output";
               type = "read";
               width = "1";
               Is_Enabled = "1";
            }
            PORT i_readdata
            {
               direction = "input";
               type = "readdata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT i_waitrequest
            {
               direction = "input";
               type = "waitrequest";
               width = "1";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Has_IRQ = "0";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-0";
            Is_Enabled = "1";
            Maximum_Burst_Size = "1";
            Burst_On_Burst_Boundaries_Only = "0";
            Linewrap_Bursts = "1";
            Interleave_Bursts = "0";
            Is_Readable = "1";
            Is_Writeable = "0";
            Address_Group = "0";
         }
      }
      MASTER data_master
      {
         PORT_WIRING 
         {
            PORT clk
            {
               direction = "input";
               type = "clk";
               width = "1";
               Is_Enabled = "1";
            }
            PORT d_address
            {
               direction = "output";
               type = "address";
               width = "23";
               Is_Enabled = "1";
            }
            PORT d_byteenable
            {
               direction = "output";
               type = "byteenable";
               width = "4";
               Is_Enabled = "1";
            }
            PORT d_irq
            {
               direction = "input";
               type = "irq";
               width = "32";
               Is_Enabled = "1";
            }
            PORT d_read
            {
               direction = "output";
               type = "read";
               width = "1";
               Is_Enabled = "1";
            }
            PORT d_readdata
            {
               direction = "input";
               type = "readdata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT d_waitrequest
            {
               direction = "input";
               type = "waitrequest";
               width = "1";
               Is_Enabled = "1";
            }
            PORT d_write
            {
               direction = "output";
               type = "write";
               width = "1";
               Is_Enabled = "1";
            }
            PORT d_writedata
            {
               direction = "output";
               type = "writedata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               direction = "input";
               type = "reset_n";
               width = "1";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "1";
            Irq_Scheme = "individual_requests";
            Interrupt_Range = "0-31";
            Is_Enabled = "1";
            Maximum_Burst_Size = "1";
            Burst_On_Burst_Boundaries_Only = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      SLAVE jtag_debug_module
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Read_Wait_States = "1";
            Write_Wait_States = "1";
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Address_Width = "9";
            Accepts_Internal_Connections = "1";
            Requires_Internal_Connections = "instruction_master,data_master";
            Accepts_External_Connections = "0";
            Is_Enabled = "0";
            Address_Alignment = "dynamic";
            Base_Address = "";
            Is_Memory_Device = "1";
            Is_Printable_Device = "0";
            Uses_Tri_State_Data_Bus = "0";
            Has_IRQ = "0";
            JTAG_Hub_Base_Id = "1118278";
            JTAG_Hub_Instance_Id = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         asp_debug = "0";
         asp_core_debug = "0";
         CPU_Architecture = "nios2";
         do_generate = "1";
         cpu_selection = "e";
         CPU_Implementation = "tiny";
         cache_has_dcache = "0";
         cache_has_icache = "0";
         cache_dcache_size = "2048";
         cache_icache_size = "4096";
         include_debug = "0";
         include_trace = "0";
         include_oci = "0";
         debug_level = "1";
         oci_offchip_trace = "0";
         oci_onchip_trace = "0";
         oci_data_trace = "0";
         oci_trace_addr_width = "7";
         oci_num_xbrk = "0";
         oci_num_dbrk = "0";
         oci_dbrk_trace = "0";
         oci_dbrk_pairs = "0";
         oci_num_pm = "0";
         oci_pm_width = "40";
         oci_debugreq_signals = "0";
         oci_instance_number = "1";
         hardware_multiply_present = "0";
         hardware_divide_present = "0";
         bht_ptr_sz = "8";
         reset_slave = "firmware_ROM/s1";
         reset_offset = "0x0";
         exc_slave = "firmware_ROM/s1";
         exc_offset = "0x00000020";
         break_slave = "firmware_ROM/s1";
         break_offset = "0x0";
         break_slave_override = "";
         break_offset_override = "0x20";
         legacy_sdk_support = "0";
         altera_internal_test = "0";
         full_waveform_signals = "0";
         activate_model_checker = "0";
         activate_monitors_and_trace = "0";
         bit_31_bypass_dcache = "1";
         always_bypass_dcache = "0";
         always_encrypt = "1";
         hdl_sim_caches_cleared = "1";
         allow_full_address_range = "0";
         consistent_synthesis = "0";
         ibuf_ptr_sz = "4";
         jtb_ptr_sz = "5";
         performance_counters_present = "0";
         performance_counters_width = "32";
         ras_ptr_sz = "4";
         inst_decode_in_submodule = "0";
         register_dependency_in_submodule = "0";
         source_operands_in_submodule = "0";
         alu_in_submodule = "0";
         stdata_in_submodule = "0";
         shift_rot_2N_in_submodule = "0";
         control_regs_in_submodule = "0";
         mult_cell_in_submodule = "0";
         M_inst_result_mux_in_submodule = "0";
         dcache_load_aligner_in_submodule = "0";
         hardware_divide_in_submodule = "0";
         mult_result_mux_in_submodule = "0";
         shift_rotate_in_submodule = "0";
         register_file_write_data_mux_in_submodule = "0";
         avalon_imaster_in_submodule = "0";
         avalon_dmaster_in_submodule = "0";
         avalon_load_aligner_in_submodule = "0";
         hbreak_test = "0";
         iss_trace_on = "0";
         iss_trace_warning = "1";
         iss_trace_info = "1";
         iss_trace_disassembly = "0";
         iss_trace_registers = "0";
         iss_trace_instr_count = "0";
         iss_software_debug = "0";
         iss_software_debug_port = "9996";
         iss_memory_dump_start = "";
         iss_memory_dump_end = "";
         Boot_Copier = "boot_loader_cfi.srec";
         Boot_Copier_EPCS = "boot_loader_epcs.srec";
         CONSTANTS 
         {
            CONSTANT __nios_catch_irqs__
            {
               value = "1";
               comment = "Include panic handler for all irqs (needs uart)";
            }
            CONSTANT __nios_use_constructors__
            {
               value = "1";
               comment = "Call c++ static constructors";
            }
            CONSTANT __nios_use_small_printf__
            {
               value = "1";
               comment = "Smaller non-ANSI printf, with no floating point";
            }
            CONSTANT nasys_has_icache
            {
               value = "0";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_icache_size
            {
               value = "4096";
               comment = "Size in bytes of instruction cache";
            }
            CONSTANT nasys_icache_line_size
            {
               value = "32";
               comment = "Size in bytes of each icache line";
            }
            CONSTANT nasys_icache_line_size_log2
            {
               value = "5";
               comment = "Log2 size in bytes of each icache line";
            }
            CONSTANT nasys_has_dcache
            {
               value = "0";
               comment = "True if instruction cache present";
            }
            CONSTANT nasys_dcache_size
            {
               value = "2048";
               comment = "Size in bytes of data cache";
            }
            CONSTANT nasys_dcache_line_size
            {
               value = "4";
               comment = "Size in bytes of each dcache line";
            }
            CONSTANT nasys_dcache_line_size_log2
            {
               value = "2";
               comment = "Log2 size in bytes of each dcache line";
            }
         }
         mainmem_slave = "";
         datamem_slave = "";
         maincomm_slave = "";
         debugcomm_slave = "";
         germs_monitor_id = "";
         remove_hardware_multiplier = "0";
         activate_trace = "1";
         activate_monitors = "1";
         activate_test_end_checker = "0";
         clear_x_bits_ld_non_bypass = "1";
         gui_include_avalon_instruction_master = "1";
         gui_include_avalon_data_master = "1";
         gui_include_dcache = "1";
         gui_include_tightly_coupled_instruction_masters = "0";
         gui_include_tightly_coupled_data_masters = "0";
         gui_num_tightly_coupled_data_masters = "1";
         num_tightly_coupled_instruction_masters = "0";
         num_tightly_coupled_data_masters = "0";
         cache_dcache_line_size = "4";
         cache_icache_line_size = "32";
         cache_dcache_bursts = "0";
         cache_icache_burst_type = "none";
         include_third_party_debug_port = "0";
         oci_trigger_arming = "1";
         gui_hardware_multiply_setting = "no_mul_small_le_shift";
         hardware_multiply_uses_les = "0";
         hardware_multiply_omits_msw = "1";
         hardware_multiply_impl = "no_mul";
         altera_show_unreleased_features = "0";
         illegal_instructions_trap = "0";
         gui_branch_prediction_type = "Automatic";
         branch_prediction_type = "";
         bht_index_pc_only = "0";
         shift_rot_impl = "small_le_shift";
         mmu_present = "0";
         process_id_num_bits = "10";
         dtlb_ptr_sz = "7";
         dtlb_num_ways = "4";
         udtlb_num_entries = "6";
         itlb_ptr_sz = "7";
         itlb_num_ways = "4";
         uitlb_num_entries = "4";
         fast_tlb_miss_exc_slave = "";
         fast_tlb_miss_exc_offset = "0x00000000";
         cache_omit_dcache = "0";
         cache_omit_icache = "0";
         omit_instruction_master = "0";
         omit_data_master = "0";
         license_status = "encrypted";
         gui_num_tightly_coupled_instruction_masters = "1";
         gui_omit_avalon_data_master = "0";
         cache_dcache_ram_block_type = "AUTO";
         cache_icache_ram_block_type = "AUTO";
         oci_embedded_pll = "1";
         gui_hardware_divide_setting = "";
         cpuid_sz = "1";
         cpuid_value = "0";
      }
      SYSTEM_BUILDER_INFO 
      {
         Parameters_Signature = "";
         Is_CPU = "1";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "STRATIX,STRATIXII,CYCLONE,CYCLONEII";
         Default_Module_Name = "cpu";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "0";
            Settings_Summary = "Nios II/e
            
            
            
            ";
         }
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
      }
      SOFTWARE_COMPONENT altera_nios2_test
      {
         class = "altera_nios2_test";
         class_version = "2.0";
         WIZARD_SCRIPT_ARGUMENTS 
         {
            CONSTANTS 
            {
               CONSTANT debug_on
               {
                  value = "0";
                  comment = "Enable debug features";
               }
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Is_Enabled = "0";
         }
      }
      SOFTWARE_COMPONENT altera_plugs_library
      {
         class = "altera_plugs_library";
         class_version = "2.1";
         WIZARD_SCRIPT_ARGUMENTS 
         {
            CONSTANTS 
            {
               CONSTANT PLUGS_PLUG_COUNT
               {
                  value = "5";
                  comment = "Maximum number of plugs";
               }
               CONSTANT PLUGS_ADAPTER_COUNT
               {
                  value = "2";
                  comment = "Maximum number of adapters";
               }
               CONSTANT PLUGS_DNS
               {
                  value = "1";
                  comment = "Have routines for DNS lookups";
               }
               CONSTANT PLUGS_PING
               {
                  value = "1";
                  comment = "Respond to icmp echo (ping) messages";
               }
               CONSTANT PLUGS_TCP
               {
                  value = "1";
                  comment = "Support tcp in/out connections";
               }
               CONSTANT PLUGS_IRQ
               {
                  value = "1";
                  comment = "Run at interrupte level";
               }
               CONSTANT PLUGS_DEBUG
               {
                  value = "1";
                  comment = "Support debug routines";
               }
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Is_Enabled = "1";
         }
      }
      MASTER custom_instruction_master
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "nios_custom_instruction";
            Data_Width = "32";
            Address_Width = "8";
            Max_Address_Width = "8";
            Base_Address = "N/A";
            Is_Visible = "0";
            Is_Custom_Instruction = "0";
            Is_Enabled = "0";
         }
      }
      PORT_WIRING 
      {
         PORT jtag_debug_trigout
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_clk
         {
            width = "1";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT jtag_debug_offchip_trace_data
         {
            width = "18";
            direction = "output";
            Is_Enabled = "0";
         }
         PORT clkx2
         {
            width = "1";
            direction = "input";
            Is_Enabled = "0";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL aaa
            {
               format = "Logic";
               name = "d_irq";
               radix = "hexadecimal";
            }
            SIGNAL aab
            {
               format = "Logic";
               name = "d_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aac
            {
               format = "Logic";
               name = "d_address";
               radix = "hexadecimal";
            }
            SIGNAL aad
            {
               format = "Logic";
               name = "d_byteenable";
               radix = "hexadecimal";
            }
            SIGNAL aae
            {
               format = "Logic";
               name = "d_read";
               radix = "hexadecimal";
            }
            SIGNAL aaf
            {
               format = "Logic";
               name = "d_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aag
            {
               format = "Logic";
               name = "d_write";
               radix = "hexadecimal";
            }
            SIGNAL aah
            {
               format = "Logic";
               name = "d_writedata";
               radix = "hexadecimal";
            }
            SIGNAL aai
            {
               format = "Logic";
               name = "i_waitrequest";
               radix = "hexadecimal";
            }
            SIGNAL aaj
            {
               format = "Logic";
               name = "i_address";
               radix = "hexadecimal";
            }
            SIGNAL aak
            {
               format = "Logic";
               name = "i_read";
               radix = "hexadecimal";
            }
            SIGNAL aal
            {
               format = "Logic";
               name = "i_readdata";
               radix = "hexadecimal";
            }
            SIGNAL aam
            {
               format = "Divider";
               name = "common";
               radix = "";
            }
            SIGNAL aan
            {
               format = "Logic";
               name = "clk";
               radix = "hexadecimal";
            }
            SIGNAL aao
            {
               format = "Logic";
               name = "reset_n";
               radix = "hexadecimal";
            }
            SIGNAL aap
            {
               format = "Logic";
               name = "F_pcb_nxt";
               radix = "hexadecimal";
            }
            SIGNAL aaq
            {
               format = "Logic";
               name = "F_pcb";
               radix = "hexadecimal";
            }
            SIGNAL aar
            {
               format = "Logic";
               name = "F_vinst";
               radix = "ascii";
            }
            SIGNAL aas
            {
               format = "Logic";
               name = "D_vinst";
               radix = "ascii";
            }
            SIGNAL aat
            {
               format = "Logic";
               name = "R_vinst";
               radix = "ascii";
            }
            SIGNAL aau
            {
               format = "Logic";
               name = "E_vinst";
               radix = "ascii";
            }
            SIGNAL aav
            {
               format = "Logic";
               name = "W_vinst";
               radix = "ascii";
            }
            SIGNAL aaw
            {
               format = "Logic";
               name = "F_valid";
               radix = "hexadecimal";
            }
            SIGNAL aax
            {
               format = "Logic";
               name = "D_valid";
               radix = "hexadecimal";
            }
            SIGNAL aay
            {
               format = "Logic";
               name = "R_valid";
               radix = "hexadecimal";
            }
            SIGNAL aaz
            {
               format = "Logic";
               name = "E_valid";
               radix = "hexadecimal";
            }
            SIGNAL aba
            {
               format = "Logic";
               name = "W_valid";
               radix = "hexadecimal";
            }
            SIGNAL abb
            {
               format = "Logic";
               name = "D_wr_dst_reg";
               radix = "hexadecimal";
            }
            SIGNAL abc
            {
               format = "Logic";
               name = "D_dst_regnum";
               radix = "hexadecimal";
            }
            SIGNAL abd
            {
               format = "Logic";
               name = "W_wr_data";
               radix = "hexadecimal";
            }
            SIGNAL abe
            {
               format = "Logic";
               name = "F_iw";
               radix = "hexadecimal";
            }
            SIGNAL abf
            {
               format = "Logic";
               name = "D_iw";
               radix = "hexadecimal";
            }
         }
      }
      MASTER tightly_coupled_instruction_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Instruction_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER data_master2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "1";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      MASTER tightly_coupled_data_master_0
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      MASTER tightly_coupled_data_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      MASTER tightly_coupled_data_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      MASTER tightly_coupled_data_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Is_Data_Master = "1";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
            Address_Group = "0";
            Is_Readable = "1";
            Is_Writeable = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_1
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
      MASTER tightly_coupled_instruction_master_3
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Register_Incoming_Signals = "0";
            Bus_Type = "avalon";
            Data_Width = "32";
            Max_Address_Width = "31";
            Address_Width = "8";
            Address_Group = "0";
            Is_Instruction_Master = "1";
            Is_Readable = "1";
            Is_Writeable = "0";
            Has_IRQ = "0";
            Is_Enabled = "0";
            Connection_Limit = "1";
            Is_Channel = "1";
         }
      }
   }
   MODULE firmware_ROM
   {
      class = "altera_avalon_onchip_memory2";
      class_version = "5.0";
      iss_model_name = "altera_memory";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/firmware_ROM.v";
         Synthesis_Only_Files = "";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         allow_mram_sim_contents_only_file = "0";
         ram_block_type = "M4K";
         gui_ram_block_type = "Automatic";
         Writeable = "0";
         dual_port = "0";
         Size_Value = "3584";
         Size_Multiple = "1";
         contents_info = "";
         MAKE 
         {
            TARGET delete_placeholder_warning
            {
               firmware_ROM 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET hex
            {
               firmware_ROM 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2hex $(ELF) 0x00000000 0xDFF --width=32 $(QUARTUS_PROJECT_DIR)/firmware_ROM.hex --create-lanes=0";
                  Dependency = "$(ELF)";
                  Target_File = "$(QUARTUS_PROJECT_DIR)/firmware_ROM.hex";
               }
            }
            TARGET sim
            {
               firmware_ROM 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Prohibited_Device_Family = "MERCURY, APEX20K, APEX20KE, APEX20KC, APEXII, ACEX1K, FLEX10KE, EXCALIBUR_ARM, MAXII";
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "onchip_memory";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "0";
         }
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               direction = "input";
               type = "address";
               width = "10";
               Is_Enabled = "1";
            }
            PORT byteenable
            {
               direction = "input";
               type = "byteenable";
               width = "4";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               direction = "input";
               type = "chipselect";
               width = "1";
               Is_Enabled = "1";
            }
            PORT clk
            {
               direction = "input";
               type = "clk";
               width = "1";
               Is_Enabled = "1";
            }
            PORT debugaccess
            {
               direction = "input";
               type = "debugaccess";
               width = "1";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               direction = "output";
               type = "readdata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT write
            {
               direction = "input";
               type = "write";
               width = "1";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               direction = "input";
               type = "writedata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT clken
            {
               Is_Enabled = "1";
               default_value = "1'b1";
               direction = "input";
               type = "clken";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "10";
            Data_Width = "32";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "3584";
            Read_Latency = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x00000000";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Base_Locked = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SLAVE s2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "10";
            Data_Width = "32";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "3584";
            Read_Latency = "1";
            Is_Enabled = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "chipselect";
               conditional = "1";
            }
            SIGNAL b
            {
               name = "write";
               conditional = "1";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "byteenable";
               radix = "binary";
               conditional = "1";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL f
            {
               name = "writedata";
               radix = "hexadecimal";
               conditional = "1";
            }
         }
      }
      PORT_WIRING 
      {
      }
   }
   MODULE data_RAM
   {
      class = "altera_avalon_onchip_memory2";
      class_version = "5.0";
      iss_model_name = "altera_memory";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/data_RAM.v";
         Synthesis_Only_Files = "";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         allow_mram_sim_contents_only_file = "0";
         ram_block_type = "M4K";
         gui_ram_block_type = "Automatic";
         Writeable = "1";
         dual_port = "0";
         Size_Value = "1";
         Size_Multiple = "1024";
         contents_info = "QUARTUS_PROJECT_DIR/data_RAM.hex 1130861912 ";
         MAKE 
         {
            TARGET delete_placeholder_warning
            {
               data_RAM 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET hex
            {
               data_RAM 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2hex $(ELF) 0x00010000 0x103FF --width=32 $(QUARTUS_PROJECT_DIR)/data_RAM.hex --create-lanes=0";
                  Dependency = "$(ELF)";
                  Target_File = "$(QUARTUS_PROJECT_DIR)/data_RAM.hex";
               }
            }
            TARGET sim
            {
               data_RAM 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Prohibited_Device_Family = "MERCURY, APEX20K, APEX20KE, APEX20KC, APEXII, ACEX1K, FLEX10KE, EXCALIBUR_ARM, MAXII";
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "onchip_memory";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "0";
         }
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               direction = "input";
               type = "address";
               width = "8";
               Is_Enabled = "1";
            }
            PORT byteenable
            {
               direction = "input";
               type = "byteenable";
               width = "4";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               direction = "input";
               type = "chipselect";
               width = "1";
               Is_Enabled = "1";
            }
            PORT clk
            {
               direction = "input";
               type = "clk";
               width = "1";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               direction = "output";
               type = "readdata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT write
            {
               direction = "input";
               type = "write";
               width = "1";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               direction = "input";
               type = "writedata";
               width = "32";
               Is_Enabled = "1";
            }
            PORT clken
            {
               Is_Enabled = "1";
               default_value = "1'b1";
               direction = "input";
               type = "clken";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "8";
            Data_Width = "32";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "1024";
            Read_Latency = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x00005000";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Base_Locked = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SLAVE s2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "8";
            Data_Width = "32";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "1024";
            Read_Latency = "1";
            Is_Enabled = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "chipselect";
               conditional = "1";
            }
            SIGNAL b
            {
               name = "write";
               conditional = "1";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "byteenable";
               radix = "binary";
               conditional = "1";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL f
            {
               name = "writedata";
               radix = "hexadecimal";
               conditional = "1";
            }
         }
      }
      PORT_WIRING 
      {
      }
   }
   MODULE payload_buffer
   {
      class = "altera_avalon_onchip_memory2";
      class_version = "5.0";
      iss_model_name = "altera_memory";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/payload_buffer.v";
         Synthesis_Only_Files = "";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         allow_mram_sim_contents_only_file = "0";
         ram_block_type = "M4K";
         gui_ram_block_type = "Automatic";
         Writeable = "1";
         dual_port = "0";
         Size_Value = "16384";
         Size_Multiple = "1";
         contents_info = "QUARTUS_PROJECT_DIR/payload_buffer.hex 1130861913 ";
         MAKE 
         {
            TARGET delete_placeholder_warning
            {
               payload_buffer 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET hex
            {
               payload_buffer 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2hex $(ELF) 0x00020000 0x23FFF --width=16 $(QUARTUS_PROJECT_DIR)/payload_buffer.hex --create-lanes=0";
                  Dependency = "$(ELF)";
                  Target_File = "$(QUARTUS_PROJECT_DIR)/payload_buffer.hex";
               }
            }
            TARGET sim
            {
               payload_buffer 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Prohibited_Device_Family = "MERCURY, APEX20K, APEX20KE, APEX20KC, APEXII, ACEX1K, FLEX10KE, EXCALIBUR_ARM, MAXII";
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Default_Module_Name = "onchip_memory";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT address
            {
               direction = "input";
               type = "address";
               width = "13";
               Is_Enabled = "1";
            }
            PORT byteenable
            {
               direction = "input";
               type = "byteenable";
               width = "2";
               Is_Enabled = "1";
            }
            PORT chipselect
            {
               direction = "input";
               type = "chipselect";
               width = "1";
               Is_Enabled = "1";
            }
            PORT clk
            {
               direction = "input";
               type = "clk";
               width = "1";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               direction = "output";
               type = "readdata";
               width = "16";
               Is_Enabled = "1";
            }
            PORT write
            {
               direction = "input";
               type = "write";
               width = "1";
               Is_Enabled = "1";
            }
            PORT writedata
            {
               direction = "input";
               type = "writedata";
               width = "16";
               Is_Enabled = "1";
            }
            PORT clken
            {
               Is_Enabled = "1";
               default_value = "1'b1";
               direction = "input";
               type = "clken";
               width = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "13";
            Data_Width = "16";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "16384";
            Read_Latency = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            Base_Address = "0x00000000";
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Base_Locked = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SLAVE s2
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Address_Width = "13";
            Data_Width = "16";
            Has_IRQ = "0";
            Read_Wait_States = "0";
            Write_Wait_States = "0";
            Address_Span = "16384";
            Read_Latency = "1";
            Is_Enabled = "0";
            Is_Channel = "1";
            Is_Writable = "1";
         }
      }
      SIMULATION 
      {
         DISPLAY 
         {
            SIGNAL a
            {
               name = "chipselect";
               conditional = "1";
            }
            SIGNAL b
            {
               name = "write";
               conditional = "1";
            }
            SIGNAL c
            {
               name = "address";
               radix = "hexadecimal";
            }
            SIGNAL d
            {
               name = "byteenable";
               radix = "binary";
               conditional = "1";
            }
            SIGNAL e
            {
               name = "readdata";
               radix = "hexadecimal";
            }
            SIGNAL f
            {
               name = "writedata";
               radix = "hexadecimal";
               conditional = "1";
            }
         }
      }
      PORT_WIRING 
      {
      }
   }
   MODULE jtag_uart_0
   {
      class = "altera_avalon_jtag_uart";
      class_version = "1.0";
      iss_model_name = "altera_avalon_jtag_uart";
      SLAVE avalon_jtag_slave
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Printable_Device = "1";
            Address_Alignment = "native";
            Address_Width = "1";
            Data_Width = "32";
            Has_IRQ = "1";
            Read_Wait_States = "peripheral_controlled";
            Write_Wait_States = "peripheral_controlled";
            JTAG_Hub_Base_Id = "0x04006E";
            JTAG_Hub_Instance_Id = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "0";
            }
            Base_Address = "0x00030000";
            Is_Base_Locked = "1";
            Connection_Limit = "1";
         }
         PORT_WIRING 
         {
            PORT clk
            {
               type = "clk";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT rst_n
            {
               type = "reset_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_chipselect
            {
               type = "chipselect";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_address
            {
               type = "address";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_read_n
            {
               type = "read_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_readdata
            {
               type = "readdata";
               direction = "output";
               width = "32";
               Is_Enabled = "1";
            }
            PORT av_write_n
            {
               type = "write_n";
               direction = "input";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_writedata
            {
               type = "writedata";
               direction = "input";
               width = "32";
               Is_Enabled = "1";
            }
            PORT av_waitrequest
            {
               type = "waitrequest";
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT av_irq
            {
               type = "irq";
               direction = "output";
               width = "1";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               Is_Enabled = "1";
               direction = "output";
               type = "dataavailable";
               width = "1";
            }
            PORT readyfordata
            {
               Is_Enabled = "1";
               direction = "output";
               type = "readyfordata";
               width = "1";
            }
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Iss_Launch_Telnet = "0";
         Clock_Source = "clk";
         View 
         {
            Settings_Summary = "<br>Write Depth: 64; Write IRQ Threshold: 8
                <br>Read  Depth: 64; Read  IRQ Threshold: 8";
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
         Top_Level_Ports_Are_Enumerated = "1";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         write_depth = "64";
         read_depth = "64";
         write_threshold = "8";
         read_threshold = "8";
         read_char_stream = "";
         showascii = "1";
         read_le = "0";
         write_le = "0";
      }
      SIMULATION 
      {
         Fix_Me_Up = "";
         DISPLAY 
         {
            SIGNAL av_chipselect
            {
               name = "av_chipselect";
            }
            SIGNAL av_address
            {
               name = "av_address";
               radix = "hexadecimal";
            }
            SIGNAL av_read_n
            {
               name = "av_read_n";
            }
            SIGNAL av_readdata
            {
               name = "av_readdata";
               radix = "hexadecimal";
            }
            SIGNAL av_write_n
            {
               name = "av_write_n";
            }
            SIGNAL av_writedata
            {
               name = "av_writedata";
               radix = "hexadecimal";
            }
            SIGNAL av_waitrequest
            {
               name = "av_waitrequest";
            }
            SIGNAL av_irq
            {
               name = "av_irq";
            }
            SIGNAL dataavailable
            {
               name = "dataavailable";
            }
            SIGNAL readyfordata
            {
               name = "readyfordata";
            }
         }
         INTERACTIVE_IN drive
         {
            enable = "0";
            file = "_input_data_stream.dat";
            mutex = "_input_data_mutex.dat";
            log = "_in.log";
            rate = "100";
            signals = "temp,list";
            exe = "nios2-terminal";
         }
         INTERACTIVE_OUT log
         {
            enable = "1";
            exe = "perl -- atail-f.pl";
            file = "_output_stream.dat";
            radix = "ascii";
            signals = "temp,list";
         }
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/jtag_uart_0.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE sysid
   {
      class = "altera_avalon_sysid";
      class_version = "4.0";
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/sysid.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
      SLAVE control_slave
      {
         PORT_WIRING 
         {
            PORT address
            {
               direction = "input";
               type = "address";
               width = "1";
               Is_Enabled = "1";
            }
            PORT readdata
            {
               direction = "output";
               type = "readdata";
               width = "32";
               Is_Enabled = "1";
            }
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Has_IRQ = "0";
            Address_Width = "1";
            Data_Width = "32";
            Base_Address = "0x00040000";
            Address_Alignment = "native";
            Read_Wait_States = "1";
            Write_Wait_States = "0";
            Read_Latency = "0";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Base_Locked = "1";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Date_Modified = "";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Fixed_Module_Name = "sysid";
         View 
         {
            Settings_Summary = "System ID (at last Generate):<br> <b>313E9921</b>    (unique ID tag) <br> <b>4367955C</b> (timestamp: Wed Nov 2, 2005 @0:18 AM)";
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         value0 = "1686625497u";
         value1 = "1079118575u";
         id = "826186017u";
         timestamp = "1130861916u";
         MAKE 
         {
            TARGET verifysysid
            {
               verifysysid 
               {
                  All_Depends_On = "0";
                  Command = "nios2-download $(JTAG_CABLE)                                --sidp=0x00040000 --id=826186017 --timestamp=1130861916";
                  Is_Phony = "1";
                  Target_File = "dummy_verifysysid_file";
               }
            }
         }
      }
   }
   MODULE asmi
   {
      class = "altera_avalon_asmi";
      class_version = "2.1";
      SLAVE asmi_control_port
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Is_Nonvolatile_Storage = "1";
            Is_Printable_Device = "0";
            Address_Alignment = "native";
            Address_Width = "3";
            Data_Width = "16";
            Has_IRQ = "1";
            Read_Wait_States = "1";
            Write_Wait_States = "1";
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "1";
            }
            Base_Address = "0x00060000";
            Is_Base_Locked = "1";
         }
         PORT_WIRING 
         {
            PORT asmi_select
            {
               direction = "input";
               type = "chipselect";
               width = "1";
               Is_Enabled = "1";
            }
            PORT clk
            {
               direction = "input";
               type = "clk";
               width = "1";
               Is_Enabled = "1";
            }
            PORT data_from_cpu
            {
               direction = "input";
               type = "writedata";
               width = "16";
               Is_Enabled = "1";
            }
            PORT data_to_cpu
            {
               direction = "output";
               type = "readdata";
               width = "16";
               Is_Enabled = "1";
            }
            PORT dataavailable
            {
               direction = "output";
               type = "dataavailable";
               width = "1";
               Is_Enabled = "1";
            }
            PORT endofpacket
            {
               direction = "output";
               type = "endofpacket";
               width = "1";
               Is_Enabled = "1";
            }
            PORT irq
            {
               direction = "output";
               type = "irq";
               width = "1";
               Is_Enabled = "1";
            }
            PORT mem_addr
            {
               direction = "input";
               type = "address";
               width = "3";
               Is_Enabled = "1";
            }
            PORT read_n
            {
               direction = "input";
               type = "read_n";
               width = "1";
               Is_Enabled = "1";
            }
            PORT readyfordata
            {
               direction = "output";
               type = "readyfordata";
               width = "1";
               Is_Enabled = "1";
            }
            PORT reset_n
            {
               direction = "input";
               type = "reset_n";
               width = "1";
               Is_Enabled = "1";
            }
            PORT write_n
            {
               direction = "input";
               type = "write_n";
               width = "1";
               Is_Enabled = "1";
            }
         }
         WIZARD_SCRIPT_ARGUMENTS 
         {
            class = "altera_avalon_asmi";
            flash_reference_designator = "U30";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Required_Device_Family = "CYCLONE,CYCLONEII,STRATIXII";
         Fixed_Module_Name = "asmi";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
         Clock_Source = "clk";
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         databits = "8";
         targetclock = "20";
         clockunits = "MHz";
         clockmult = "1000000";
         numslaves = "1";
         ismaster = "1";
         clockpolarity = "0";
         clockphase = "0";
         lsbfirst = "0";
         extradelay = "0";
         targetssdelay = "100";
         delayunits = "us";
         delaymult = "1e-006";
         prefix = "asmi_";
         CONSTANTS 
         {
            CONSTANT na_asmi_64K
            {
               value = "0";
               comment = "ASMI part is 64k bits";
            }
            CONSTANT na_asmi_1M
            {
               value = "0";
               comment = "ASMI part is 1M bits";
            }
            CONSTANT na_asmi_4M
            {
               value = "1";
               comment = "ASMI part is 4M bits";
            }
         }
         clockunit = "kHz";
         delayunit = "us";
      }
      HDL_INFO 
      {
         Precompiled_Simulation_Library_Files = "";
         Simulation_HDL_Files = "";
         Synthesis_HDL_Files = "__PROJECT_DIRECTORY__/asmi.v";
         Synthesis_Only_Files = "";
      }
      PORT_WIRING 
      {
      }
   }
   MODULE Board_System
   {
      class = "altera_user_board_setup";
      class_version = "1.0";
      SLAVE bogus_slave
      {
         PORT_WIRING 
         {
         }
         SYSTEM_BUILDER_INFO 
         {
            Is_Enabled = "0";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Component_Name = "DE2_Board";
         JTAG_device_index = "1";
         name1 = "EPSC16";
         slave1 = "asmi/asmi_control_port";
         offset1 = "0x00000000";
         length1 = "";
         name2 = "FLASH";
         slave2 = "cfi_flash_0/s1";
         offset2 = "0x00000000";
         length2 = "";
         name3 = "";
         slave3 = "";
         offset3 = "";
         length3 = "";
         name4 = "";
         slave4 = "";
         offset4 = "";
         length4 = "";
         name5 = "";
         slave5 = "";
         offset5 = "";
         length5 = "";
         name6 = "";
         slave6 = "";
         offset6 = "";
         length6 = "";
         name7 = "";
         slave7 = "";
         offset7 = "";
         length7 = "";
         name8 = "";
         slave8 = "";
         offset8 = "";
         length8 = "";
      }
      SYSTEM_BUILDER_INFO 
      {
         Is_Enabled = "1";
         Instantiate_In_System_Module = "1";
         Fixed_Module_Name = "Board_System";
         Is_Visible = "0";
         View 
         {
            Is_Collapsed = "1";
            MESSAGES 
            {
            }
         }
         Clock_Source = "clk";
      }
   }
   MODULE tri_state_bridge_0
   {
      class = "altera_avalon_tri_state_bridge";
      class_version = "2.0";
      SLAVE avalon_slave
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon";
            Bridges_To = "tristate_master";
            Base_Address = "N/A";
            Has_IRQ = "0";
            IRQ = "N/A";
            Register_Outgoing_Signals = "1";
            Register_Incoming_Signals = "1";
            MASTERED_BY cpu_0/instruction_master
            {
               priority = "1";
            }
            MASTERED_BY cpu_0/data_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
         }
      }
      MASTER tristate_master
      {
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon_tristate";
            Bridges_To = "avalon_slave";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Instantiate_In_System_Module = "1";
         Is_Enabled = "1";
         Is_Bridge = "1";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "0";
         }
      }
   }
   MODULE cfi_flash_0
   {
      class = "altera_avalon_cfi_flash";
      class_version = "1.1";
      iss_model_name = "altera_avalon_flash";
      HDL_INFO 
      {
      }
      SLAVE s1
      {
         PORT_WIRING 
         {
            PORT data
            {
               width = "8";
               is_shared = "1";
               direction = "inout";
               type = "data";
            }
            PORT address
            {
               width = "22";
               is_shared = "1";
               direction = "input";
               type = "address";
            }
            PORT read_n
            {
               width = "1";
               is_shared = "1";
               direction = "input";
               type = "read_n";
            }
            PORT write_n
            {
               width = "1";
               is_shared = "0";
               direction = "input";
               type = "write_n";
            }
            PORT select_n
            {
               width = "1";
               is_shared = "0";
               direction = "input";
               type = "chipselect_n";
            }
         }
         WIZARD_SCRIPT_ARGUMENTS 
         {
            class = "altera_avalon_cfi_flash";
            Supports_Flash_File_System = "1";
            flash_reference_designator = "U20";
         }
         SYSTEM_BUILDER_INFO 
         {
            Bus_Type = "avalon_tristate";
            Is_Nonvolatile_Storage = "1";
            Is_Memory_Device = "1";
            Address_Alignment = "dynamic";
            Has_IRQ = "0";
            Base_Address = "0x00100000";
            Data_Width = "8";
            Address_Width = "22";
            Simulation_Num_Lanes = "1";
            Convert_Xs_To_0 = "1";
            Write_Wait_States = "160ns";
            Read_Wait_States = "160ns";
            Setup_Time = "160ns";
            Hold_Time = "160ns";
            Address_Span = "4194304";
            MASTERED_BY tri_state_bridge_0/tristate_master
            {
               priority = "1";
            }
            IRQ_MASTER cpu_0/data_master
            {
               IRQ_Number = "NC";
            }
            Is_Base_Locked = "1";
         }
      }
      SYSTEM_BUILDER_INFO 
      {
         Make_Memory_Model = "1";
         Is_Enabled = "1";
         Instantiate_In_System_Module = "0";
         Top_Level_Ports_Are_Enumerated = "1";
         Clock_Source = "clk";
         View 
         {
            MESSAGES 
            {
            }
            Is_Collapsed = "1";
         }
      }
      WIZARD_SCRIPT_ARGUMENTS 
      {
         Setup_Value = "160";
         Wait_Value = "160";
         Hold_Value = "160";
         Timing_Units = "ns";
         Unit_Multiplier = "1";
         Size = "4194304";
         MAKE 
         {
            MACRO 
            {
               CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX = "$(CFI_FLASH_0_FLASHTARGET_TMP1:0=)";
               CFI_FLASH_0_FLASHTARGET_TMP1 = "$(ALT_SIM_OPTIMIZE:1=RUN_ON_HDL_SIMULATOR_ONLY_)";
            }
            MASTER cpu_0
            {
               MACRO 
               {
                  BOOT_COPIER = "boot_loader_cfi.srec";
                  CPU_CLASS = "altera_nios2";
                  CPU_RESET_ADDRESS = "0x0";
               }
            }
            TARGET delete_placeholder_warning
            {
               cfi_flash_0 
               {
                  Command1 = "rm -f $(SIMDIR)/contents_file_warning.txt";
                  Is_Phony = "1";
                  Target_File = "do_delete_placeholder_warning";
               }
            }
            TARGET flashfiles
            {
               cfi_flash_0 
               {
                  Command1 = "@echo Post-processing to create $(notdir $@)";
                  Command2 = "elf2flash --input=$(ELF) --flash=U20 --boot=$(shell $(QUARTUS_ROOTDIR)/sopc_builder/bin/find_sopc_component_dir $(CPU_CLASS))/$(BOOT_COPIER) --outfile=$(CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX)cfi_flash_0.flash --sim_optimize=$(ALT_SIM_OPTIMIZE) --base=0x400000 --end=0x7FFFFF --reset=$(CPU_RESET_ADDRESS) ";
                  Dependency = "$(ELF)";
                  Target_File = "$(CFI_FLASH_0_FLASHTARGET_ALT_SIM_PREFIX)cfi_flash_0.flash";
               }
            }
            TARGET sim
            {
               cfi_flash_0 
               {
                  Command1 = "if [ ! -d $(SIMDIR) ]; then mkdir $(SIMDIR) ; fi";
                  Command2 = "@echo Hardware simulation is not enabled for the target SOPC Builder system. Skipping creation of hardware simulation model contents and simulation symbol files. \\(Note: This does not affect the instruction set simulator.\\)";
                  Command3 = "touch $(SIMDIR)/dummy_file";
                  Dependency = "$(ELF)";
                  Target_File = "$(SIMDIR)/dummy_file";
               }
            }
         }
      }
   }
}
