--------------------------------------------------------------------------------------
Timing Analyzer Summary
--------------------------------------------------------------------------------------

Type           : Worst-case tsu
Slack          : N/A
Required Time  : None
Actual Time    : 10.431 ns
From           : SRAM_DQ[5]
To             : system_0:u0|cpu_0:the_cpu_0|d_readdata_d1[21]
From Clock     : --
To Clock       : CLOCK_50
Failed Paths   : 0

Type           : Worst-case tco
Slack          : N/A
Required Time  : None
Actual Time    : 15.450 ns
From           : system_0:u0|Audio_0:the_Audio_0|AUDIO_DAC_FIFO:the_AUDIO_DAC_FIFO|SEL_Cont[3]
To             : AUD_DACDAT
From Clock     : CLOCK_27
To Clock       : --
Failed Paths   : 0

Type           : Worst-case tpd
Slack          : N/A
Required Time  : None
Actual Time    : 2.612 ns
From           : altera_internal_jtag~TDO
To             : altera_reserved_tdo
From Clock     : --
To Clock       : --
Failed Paths   : 0

Type           : Worst-case th
Slack          : N/A
Required Time  : None
Actual Time    : 3.877 ns
From           : altera_internal_jtag~TMSUTAP
To             : sld_hub:sld_hub_inst|sld_jtag_state_machine:jtag_state_machine|tms_cnt[0]
From Clock     : --
To Clock       : altera_internal_jtag~TCKUTAP
Failed Paths   : 0

Type           : Clock Setup: 'SDRAM_PLL:PLL1|altpll:altpll_component|_clk1'
Slack          : 0.758 ns
Required Time  : 100.00 MHz ( period = 10.000 ns )
Actual Time    : 108.20 MHz ( period = 9.242 ns )
From           : system_0:u0|cpu_0:the_cpu_0|d_address[20]
To             : system_0:u0|cpu_0:the_cpu_0|d_readdata_d1[4]
From Clock     : SDRAM_PLL:PLL1|altpll:altpll_component|_clk1
To Clock       : SDRAM_PLL:PLL1|altpll:altpll_component|_clk1
Failed Paths   : 0

Type           : Clock Setup: 'SDRAM_PLL:PLL1|altpll:altpll_component|_clk2'
Slack          : 2.305 ns
Required Time  : 25.00 MHz ( period = 40.000 ns )
Actual Time    : N/A
From           : system_0:u0|VGA_0:the_VGA_0|VGA_NIOS_CTRL:the_VGA_NIOS_CTRL|mCursor_X[2]
To             : system_0:u0|VGA_0:the_VGA_0|VGA_NIOS_CTRL:the_VGA_NIOS_CTRL|VGA_Controller:u0|Cur_Color_B[1]
From Clock     : SDRAM_PLL:PLL1|altpll:altpll_component|_clk1
To Clock       : SDRAM_PLL:PLL1|altpll:altpll_component|_clk2
Failed Paths   : 0

Type           : Clock Setup: 'CLOCK_50'
Slack          : 10.074 ns
Required Time  : 50.00 MHz ( period = 20.000 ns )
Actual Time    : 100.75 MHz ( period = 9.926 ns )
From           : system_0:u0|sdram_0:the_sdram_0|sdram_0_input_efifo_module:the_sdram_0_input_efifo_module|rd_address
To             : system_0:u0|sdram_0:the_sdram_0|m_addr[6]
From Clock     : CLOCK_50
To Clock       : CLOCK_50
Failed Paths   : 0

Type           : Clock Setup: 'Audio_PLL:PLL2|altpll:altpll_component|_clk0'
Slack          : 48.612 ns
Required Time  : 18.41 MHz ( period = 54.320 ns )
Actual Time    : 175.19 MHz ( period = 5.708 ns )
From           : system_0:u0|Audio_0:the_Audio_0|AUDIO_DAC_FIFO:the_AUDIO_DAC_FIFO|FIFO_16_256:u0|dcfifo:dcfifo_component|dcfifo_9ai1:auto_generated|rdptr_g[8]
To             : system_0:u0|Audio_0:the_Audio_0|AUDIO_DAC_FIFO:the_AUDIO_DAC_FIFO|FIFO_16_256:u0|dcfifo:dcfifo_component|dcfifo_9ai1:auto_generated|a_graycounter_g86:rdptr_g1p|counter_ffa[8]
From Clock     : Audio_PLL:PLL2|altpll:altpll_component|_clk0
To Clock       : Audio_PLL:PLL2|altpll:altpll_component|_clk0
Failed Paths   : 0

Type           : Clock Setup: 'altera_internal_jtag~TCKUTAP'
Slack          : N/A
Required Time  : None
Actual Time    : 111.52 MHz ( period = 8.967 ns )
From           : sld_hub:sld_hub_inst|sld_dffex:IRF_ENA|Q[0]
To             : system_0:u0|cpu_0:the_cpu_0|cpu_0_nios2_oci:the_cpu_0_nios2_oci|cpu_0_jtag_debug_module_wrapper:the_cpu_0_jtag_debug_module_wrapper|cpu_0_jtag_debug_module:the_cpu_0_jtag_debug_module1|sr[22]
From Clock     : altera_internal_jtag~TCKUTAP
To Clock       : altera_internal_jtag~TCKUTAP
Failed Paths   : 0

Type           : Clock Hold: 'SDRAM_PLL:PLL1|altpll:altpll_component|_clk1'
Slack          : 0.391 ns
Required Time  : 100.00 MHz ( period = 10.000 ns )
Actual Time    : N/A
From           : system_0:u0|SD_CLK:the_SD_CLK|data_out
To             : system_0:u0|SD_CLK:the_SD_CLK|data_out
From Clock     : SDRAM_PLL:PLL1|altpll:altpll_component|_clk1
To Clock       : SDRAM_PLL:PLL1|altpll:altpll_component|_clk1
Failed Paths   : 0

Type           : Clock Hold: 'SDRAM_PLL:PLL1|altpll:altpll_component|_clk2'
Slack          : 0.391 ns
Required Time  : 25.00 MHz ( period = 40.000 ns )
Actual Time    : N/A
From           : system_0:u0|VGA_0:the_VGA_0|VGA_NIOS_CTRL:the_VGA_NIOS_CTRL|VGA_Controller:u0|oVGA_V_SYNC
To             : system_0:u0|VGA_0:the_VGA_0|VGA_NIOS_CTRL:the_VGA_NIOS_CTRL|VGA_Controller:u0|oVGA_V_SYNC
From Clock     : SDRAM_PLL:PLL1|altpll:altpll_component|_clk2
To Clock       : SDRAM_PLL:PLL1|altpll:altpll_component|_clk2
Failed Paths   : 0

Type           : Clock Hold: 'Audio_PLL:PLL2|altpll:altpll_component|_clk0'
Slack          : 0.391 ns
Required Time  : 18.41 MHz ( period = 54.320 ns )
Actual Time    : N/A
From           : system_0:u0|Audio_0:the_Audio_0|AUDIO_DAC_FIFO:the_AUDIO_DAC_FIFO|LRCK_1X
To             : system_0:u0|Audio_0:the_Audio_0|AUDIO_DAC_FIFO:the_AUDIO_DAC_FIFO|LRCK_1X
From Clock     : Audio_PLL:PLL2|altpll:altpll_component|_clk0
To Clock       : Audio_PLL:PLL2|altpll:altpll_component|_clk0
Failed Paths   : 0

Type           : Clock Hold: 'CLOCK_50'
Slack          : 0.391 ns
Required Time  : 50.00 MHz ( period = 20.000 ns )
Actual Time    : N/A
From           : system_0:u0|sdram_0:the_sdram_0|i_cmd[3]
To             : system_0:u0|sdram_0:the_sdram_0|i_cmd[3]
From Clock     : CLOCK_50
To Clock       : CLOCK_50
Failed Paths   : 0

Type           : Total number of failed paths
Slack          : 
Required Time  : 
Actual Time    : 
From           : 
To             : 
From Clock     : 
To Clock       : 
Failed Paths   : 0

--------------------------------------------------------------------------------------

