// megafunction wizard: %ALTPLL%
// GENERATION: STANDARD
// VERSION: WM1.0
// MODULE: altpll 

// ============================================================
// File Name: SDRAM_PLL.v
// Megafunction Name(s):
// 			altpll
// ============================================================
// ************************************************************
// THIS IS A WIZARD-GENERATED FILE. DO NOT EDIT THIS FILE!
//
// 6.0 Build 202 06/20/2006 SP 1 SJ Full Version
// ************************************************************


//Copyright (C) 1991-2006 Altera Corporation
//Your use of Altera Corporation's design tools, logic functions 
//and other software and tools, and its AMPP partner logic 
//functions, and any output files any of the foregoing 
//(including device programming or simulation files), and any 
//associated documentation or information are expressly subject 
//to the terms and conditions of the Altera Program License 
//Subscription Agreement, Altera MegaCore Function License 
//Agreement, or other applicable license agreement, including, 
//without limitation, that your use is for the sole purpose of 
//programming logic devices manufactured by Altera and sold by 
//Altera or its authorized distributors.  Please refer to the 
//applicable agreement for further details.


// synopsys translate_off
`timescale 1 ps / 1 ps
// synopsys translate_on
module SDRAM_PLL (
	inclk0,
	c0,
	c1,
	c2);

	input	  inclk0;
	output	  c0;
	output	  c1;
	output	  c2;

	wire [5:0] sub_wire0;
	wire [0:0] sub_wire6 = 1'h0;
	wire [2:2] sub_wire3 = sub_wire0[2:2];
	wire [1:1] sub_wire2 = sub_wire0[1:1];
	wire [0:0] sub_wire1 = sub_wire0[0:0];
	wire  c0 = sub_wire1;
	wire  c1 = sub_wire2;
	wire  c2 = sub_wire3;
	wire  sub_wire4 = inclk0;
	wire [1:0] sub_wire5 = {sub_wire6, sub_wire4};

	altpll	altpll_component (
				.inclk (sub_wire5),
				.clk (sub_wire0),
				.activeclock (),
				.areset (1'b0),
				.clkbad (),
				.clkena ({6{1'b1}}),
				.clkloss (),
				.clkswitch (1'b0),
				.enable0 (),
				.enable1 (),
				.extclk (),
				.extclkena ({4{1'b1}}),
				.fbin (1'b1),
				.locked (),
				.pfdena (1'b1),
				.pllena (1'b1),
				.scanaclr (1'b0),
				.scanclk (1'b0),
				.scandata (1'b0),
				.scandataout (),
				.scandone (),
				.scanread (1'b0),
				.scanwrite (1'b0),
				.sclkout0 (),
				.sclkout1 ());
	defparam
		altpll_component.clk0_divide_by = 1,
		altpll_component.clk0_duty_cycle = 50,
		altpll_component.clk0_multiply_by = 1,
		altpll_component.clk0_phase_shift = "-3000",
		altpll_component.clk1_divide_by = 1,
		altpll_component.clk1_duty_cycle = 50,
		altpll_component.clk1_multiply_by = 2,
		altpll_component.clk1_phase_shift = "0",
		altpll_component.clk2_divide_by = 2,
		altpll_component.clk2_duty_cycle = 50,
		altpll_component.clk2_multiply_by = 1,
		altpll_component.clk2_phase_shift = "0",
		altpll_component.compensate_clock = "CLK0",
		altpll_component.inclk0_input_frequency = 20000,
		altpll_component.intended_device_family = "Cyclone II",
		altpll_component.lpm_type = "altpll",
		altpll_component.operation_mode = "NORMAL",
		altpll_component.pll_type = "FAST",
		altpll_component.port_activeclock = "PORT_UNUSED",
		altpll_component.port_areset = "PORT_UNUSED",
		altpll_component.port_clkbad0 = "PORT_UNUSED",
		altpll_component.port_clkbad1 = "PORT_UNUSED",
		altpll_component.port_clkloss = "PORT_UNUSED",
		altpll_component.port_clkswitch = "PORT_UNUSED",
		altpll_component.port_fbin = "PORT_UNUSED",
		altpll_component.port_inclk0 = "PORT_USED",
		altpll_component.port_inclk1 = "PORT_UNUSED",
		altpll_component.port_locked = "PORT_UNUSED",
		altpll_component.port_pfdena = "PORT_UNUSED",
		altpll_component.port_pllena = "PORT_UNUSED",
		altpll_component.port_scanaclr = "PORT_UNUSED",
		altpll_component.port_scanclk = "PORT_UNUSED",
		altpll_component.port_scandata = "PORT_UNUSED",
		altpll_component.port_scandataout = "PORT_UNUSED",
		altpll_component.port_scandone = "PORT_UNUSED",
		altpll_component.port_scanread = "PORT_UNUSED",
		altpll_component.port_scanwrite = "PORT_UNUSED",
		altpll_component.port_clk0 = "PORT_USED",
		altpll_component.port_clk1 = "PORT_USED",
		altpll_component.port_clk2 = "PORT_USED",
		altpll_component.port_clk3 = "PORT_UNUSED",
		altpll_component.port_clk4 = "PORT_UNUSED",
		altpll_component.port_clk5 = "PORT_UNUSED",
		altpll_component.port_clkena0 = "PORT_UNUSED",
		altpll_component.port_clkena1 = "PORT_UNUSED",
		altpll_component.port_clkena2 = "PORT_UNUSED",
		altpll_component.port_clkena3 = "PORT_UNUSED",
		altpll_component.port_clkena4 = "PORT_UNUSED",
		altpll_component.port_clkena5 = "PORT_UNUSED",
		altpll_component.port_enable0 = "PORT_UNUSED",
		altpll_component.port_enable1 = "PORT_UNUSED",
		altpll_component.port_extclk0 = "PORT_UNUSED",
		altpll_component.port_extclk1 = "PORT_UNUSED",
		altpll_component.port_extclk2 = "PORT_UNUSED",
		altpll_component.port_extclk3 = "PORT_UNUSED",
		altpll_component.port_extclkena0 = "PORT_UNUSED",
		altpll_component.port_extclkena1 = "PORT_UNUSED",
		altpll_component.port_extclkena2 = "PORT_UNUSED",
		altpll_component.port_extclkena3 = "PORT_UNUSED",
		altpll_component.port_sclkout0 = "PORT_UNUSED",
		altpll_component.port_sclkout1 = "PORT_UNUSED";


endmodule

// ============================================================
// CNX file retrieval info
// ============================================================
// Retrieval info: PRIVATE: ACTIVECLK_CHECK STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH STRING "1.000"
// Retrieval info: PRIVATE: BANDWIDTH_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH_FREQ_UNIT STRING "MHz"
// Retrieval info: PRIVATE: BANDWIDTH_PRESET STRING "Low"
// Retrieval info: PRIVATE: BANDWIDTH_USE_AUTO STRING "1"
// Retrieval info: PRIVATE: BANDWIDTH_USE_CUSTOM STRING "0"
// Retrieval info: PRIVATE: BANDWIDTH_USE_PRESET STRING "0"
// Retrieval info: PRIVATE: CLKBAD_SWITCHOVER_CHECK STRING "0"
// Retrieval info: PRIVATE: CLKLOSS_CHECK STRING "0"
// Retrieval info: PRIVATE: CLKSWITCH_CHECK STRING "1"
// Retrieval info: PRIVATE: CNX_NO_COMPENSATE_RADIO STRING "0"
// Retrieval info: PRIVATE: CREATE_CLKBAD_CHECK STRING "0"
// Retrieval info: PRIVATE: CREATE_INCLK1_CHECK STRING "0"
// Retrieval info: PRIVATE: CUR_DEDICATED_CLK STRING "c0"
// Retrieval info: PRIVATE: CUR_FBIN_CLK STRING "e0"
// Retrieval info: PRIVATE: DEVICE_SPEED_GRADE STRING "Any"
// Retrieval info: PRIVATE: DEV_FAMILY STRING "Cyclone II"
// Retrieval info: PRIVATE: DIV_FACTOR0 NUMERIC "1"
// Retrieval info: PRIVATE: DIV_FACTOR1 NUMERIC "2"
// Retrieval info: PRIVATE: DIV_FACTOR2 NUMERIC "1"
// Retrieval info: PRIVATE: DUTY_CYCLE0 STRING "50.00000000"
// Retrieval info: PRIVATE: DUTY_CYCLE1 STRING "50.00000000"
// Retrieval info: PRIVATE: DUTY_CYCLE2 STRING "50.00000000"
// Retrieval info: PRIVATE: EXT_FEEDBACK_RADIO STRING "0"
// Retrieval info: PRIVATE: GLOCKED_COUNTER_EDIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: GLOCKED_FEATURE_ENABLED STRING "1"
// Retrieval info: PRIVATE: GLOCKED_MODE_CHECK STRING "0"
// Retrieval info: PRIVATE: GLOCK_COUNTER_EDIT NUMERIC "1048575"
// Retrieval info: PRIVATE: HAS_MANUAL_SWITCHOVER STRING "1"
// Retrieval info: PRIVATE: INCLK0_FREQ_EDIT STRING "50.000"
// Retrieval info: PRIVATE: INCLK0_FREQ_UNIT_COMBO STRING "MHz"
// Retrieval info: PRIVATE: INCLK1_FREQ_EDIT STRING "50.000"
// Retrieval info: PRIVATE: INCLK1_FREQ_EDIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: INCLK1_FREQ_UNIT_CHANGED STRING "1"
// Retrieval info: PRIVATE: INCLK1_FREQ_UNIT_COMBO STRING "MHz"
// Retrieval info: PRIVATE: INT_FEEDBACK__MODE_RADIO STRING "1"
// Retrieval info: PRIVATE: LOCKED_OUTPUT_CHECK STRING "0"
// Retrieval info: PRIVATE: LONG_SCAN_RADIO STRING "1"
// Retrieval info: PRIVATE: LVDS_MODE_DATA_RATE STRING "Not Available"
// Retrieval info: PRIVATE: LVDS_MODE_DATA_RATE_DIRTY NUMERIC "0"
// Retrieval info: PRIVATE: LVDS_PHASE_SHIFT_UNIT0 STRING "deg"
// Retrieval info: PRIVATE: LVDS_PHASE_SHIFT_UNIT1 STRING "ps"
// Retrieval info: PRIVATE: LVDS_PHASE_SHIFT_UNIT2 STRING "ps"
// Retrieval info: PRIVATE: MIRROR_CLK0 STRING "0"
// Retrieval info: PRIVATE: MIRROR_CLK1 STRING "0"
// Retrieval info: PRIVATE: MIRROR_CLK2 STRING "0"
// Retrieval info: PRIVATE: MULT_FACTOR0 NUMERIC "1"
// Retrieval info: PRIVATE: MULT_FACTOR1 NUMERIC "1"
// Retrieval info: PRIVATE: MULT_FACTOR2 NUMERIC "1"
// Retrieval info: PRIVATE: NORMAL_MODE_RADIO STRING "1"
// Retrieval info: PRIVATE: OUTPUT_FREQ0 STRING "50.00000000"
// Retrieval info: PRIVATE: OUTPUT_FREQ1 STRING "100.00000000"
// Retrieval info: PRIVATE: OUTPUT_FREQ2 STRING "25.00000000"
// Retrieval info: PRIVATE: OUTPUT_FREQ_MODE0 STRING "1"
// Retrieval info: PRIVATE: OUTPUT_FREQ_MODE1 STRING "1"
// Retrieval info: PRIVATE: OUTPUT_FREQ_MODE2 STRING "1"
// Retrieval info: PRIVATE: OUTPUT_FREQ_UNIT0 STRING "MHz"
// Retrieval info: PRIVATE: OUTPUT_FREQ_UNIT1 STRING "MHz"
// Retrieval info: PRIVATE: OUTPUT_FREQ_UNIT2 STRING "MHz"
// Retrieval info: PRIVATE: PHASE_SHIFT0 STRING "-3.00000000"
// Retrieval info: PRIVATE: PHASE_SHIFT1 STRING "0.00000000"
// Retrieval info: PRIVATE: PHASE_SHIFT2 STRING "0.00000000"
// Retrieval info: PRIVATE: PHASE_SHIFT_UNIT0 STRING "ns"
// Retrieval info: PRIVATE: PHASE_SHIFT_UNIT1 STRING "ps"
// Retrieval info: PRIVATE: PHASE_SHIFT_UNIT2 STRING "ps"
// Retrieval info: PRIVATE: PLL_ADVANCED_PARAM_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_ARESET_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_AUTOPLL_CHECK NUMERIC "1"
// Retrieval info: PRIVATE: PLL_ENA_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_ENHPLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_FASTPLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_LVDS_PLL_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PLL_PFDENA_CHECK STRING "0"
// Retrieval info: PRIVATE: PLL_TARGET_HARCOPY_CHECK NUMERIC "0"
// Retrieval info: PRIVATE: PRIMARY_CLK_COMBO STRING "inclk0"
// Retrieval info: PRIVATE: SACN_INPUTS_CHECK STRING "0"
// Retrieval info: PRIVATE: SCAN_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: SELF_RESET_LOCK_LOSS STRING "0"
// Retrieval info: PRIVATE: SHORT_SCAN_RADIO STRING "0"
// Retrieval info: PRIVATE: SPREAD_FEATURE_ENABLED STRING "0"
// Retrieval info: PRIVATE: SPREAD_FREQ STRING "50.000"
// Retrieval info: PRIVATE: SPREAD_FREQ_UNIT STRING "KHz"
// Retrieval info: PRIVATE: SPREAD_PERCENT STRING "0.500"
// Retrieval info: PRIVATE: SPREAD_USE STRING "0"
// Retrieval info: PRIVATE: SRC_SYNCH_COMP_RADIO STRING "0"
// Retrieval info: PRIVATE: STICKY_CLK0 STRING "1"
// Retrieval info: PRIVATE: STICKY_CLK1 STRING "1"
// Retrieval info: PRIVATE: STICKY_CLK2 STRING "1"
// Retrieval info: PRIVATE: SWITCHOVER_COUNT_EDIT NUMERIC "1"
// Retrieval info: PRIVATE: SWITCHOVER_FEATURE_ENABLED STRING "1"
// Retrieval info: PRIVATE: USE_CLK0 STRING "1"
// Retrieval info: PRIVATE: USE_CLK1 STRING "1"
// Retrieval info: PRIVATE: USE_CLK2 STRING "1"
// Retrieval info: PRIVATE: USE_CLKENA0 STRING "0"
// Retrieval info: PRIVATE: USE_CLKENA1 STRING "0"
// Retrieval info: PRIVATE: USE_CLKENA2 STRING "0"
// Retrieval info: PRIVATE: ZERO_DELAY_RADIO STRING "0"
// Retrieval info: LIBRARY: altera_mf altera_mf.altera_mf_components.all
// Retrieval info: CONSTANT: CLK0_DIVIDE_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK0_DUTY_CYCLE NUMERIC "50"
// Retrieval info: CONSTANT: CLK0_MULTIPLY_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK0_PHASE_SHIFT STRING "-3000"
// Retrieval info: CONSTANT: CLK1_DIVIDE_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK1_DUTY_CYCLE NUMERIC "50"
// Retrieval info: CONSTANT: CLK1_MULTIPLY_BY NUMERIC "2"
// Retrieval info: CONSTANT: CLK1_PHASE_SHIFT STRING "0"
// Retrieval info: CONSTANT: CLK2_DIVIDE_BY NUMERIC "2"
// Retrieval info: CONSTANT: CLK2_DUTY_CYCLE NUMERIC "50"
// Retrieval info: CONSTANT: CLK2_MULTIPLY_BY NUMERIC "1"
// Retrieval info: CONSTANT: CLK2_PHASE_SHIFT STRING "0"
// Retrieval info: CONSTANT: COMPENSATE_CLOCK STRING "CLK0"
// Retrieval info: CONSTANT: INCLK0_INPUT_FREQUENCY NUMERIC "20000"
// Retrieval info: CONSTANT: INTENDED_DEVICE_FAMILY STRING "Cyclone II"
// Retrieval info: CONSTANT: LPM_TYPE STRING "altpll"
// Retrieval info: CONSTANT: OPERATION_MODE STRING "NORMAL"
// Retrieval info: CONSTANT: PLL_TYPE STRING "FAST"
// Retrieval info: CONSTANT: PORT_ACTIVECLOCK STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_ARESET STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKBAD0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKBAD1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKLOSS STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_CLKSWITCH STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_FBIN STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_INCLK0 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_INCLK1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_LOCKED STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PFDENA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_PLLENA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANACLR STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANCLK STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDATA STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDATAOUT STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANDONE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANREAD STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_SCANWRITE STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk0 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_clk1 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_clk2 STRING "PORT_USED"
// Retrieval info: CONSTANT: PORT_clk3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk4 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clk5 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena4 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_clkena5 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_enable0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_enable1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclk3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclkena0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclkena1 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclkena2 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_extclkena3 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_sclkout0 STRING "PORT_UNUSED"
// Retrieval info: CONSTANT: PORT_sclkout1 STRING "PORT_UNUSED"
// Retrieval info: USED_PORT: @clk 0 0 6 0 OUTPUT_CLK_EXT VCC "@clk[5..0]"
// Retrieval info: USED_PORT: @extclk 0 0 4 0 OUTPUT_CLK_EXT VCC "@extclk[3..0]"
// Retrieval info: USED_PORT: c0 0 0 0 0 OUTPUT_CLK_EXT VCC "c0"
// Retrieval info: USED_PORT: c1 0 0 0 0 OUTPUT_CLK_EXT VCC "c1"
// Retrieval info: USED_PORT: c2 0 0 0 0 OUTPUT_CLK_EXT VCC "c2"
// Retrieval info: USED_PORT: inclk0 0 0 0 0 INPUT_CLK_EXT GND "inclk0"
// Retrieval info: CONNECT: @inclk 0 0 1 0 inclk0 0 0 0 0
// Retrieval info: CONNECT: c0 0 0 0 0 @clk 0 0 1 0
// Retrieval info: CONNECT: c1 0 0 0 0 @clk 0 0 1 1
// Retrieval info: CONNECT: c2 0 0 0 0 @clk 0 0 1 2
// Retrieval info: CONNECT: @inclk 0 0 1 1 GND 0 0 0 0
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL.v TRUE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL.inc FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL.cmp FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL.bsf FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL_inst.v FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL_bb.v FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL_waveforms.html FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL_wave*.jpg FALSE FALSE
// Retrieval info: GEN_FILE: TYPE_NORMAL SDRAM_PLL.ppf TRUE FALSE
